1. Clear map 1, activate map 1 (load default: snmp will become OFF)
2. Unregister all card, register all card with protection mode
3. Check all card are working
4. Construct map , adjust clock mode=SSM
5. Store configure
6. Upload configure
7. Send data path
8. Tributary card reset (MIB: cold/warm)
9. Check data path won’t unsync
10. XCU Downgrade to previous version (V1.15.01.0053)
11. XCU Upgrade to current version (V1.15.02.0001)
12. Check download version is correct
13. XCU Reset (standby cold/warm)
14. Check data path is sync., no any bit error,unsync sec.
15. XCU Reset (working warm/cold)
16. Check data path won’t unsync (working warm : no bit error , working cold: unsync sec<2)
17. Clear map 1
18. Retrieve configure
19. Send data path
20. Check data path won’t unsync
21. Power on/off
22. Send data path
23. Check data path won’t unsync